{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["配置说明","HW"],"read":"whole","date_system":"1900"}

{"sheet":"配置说明","index":0,"n_rows":2,"n_cols":1,"rows_kept":2}
["说明"]
["1-本报价有效期截止到2019年4月30日\n2-当前费用为预估，根据最终落地方案对应的具体配置可能调整\n3-当前已选择服务有规格定义，当实际使用资源超过原定规格，多使用的资源需另行计费\n4-实际价格以官网为准，实际配置以最终客户需求为准"]

{"sheet":"HW","index":1,"n_rows":19,"n_cols":9,"rows_kept":19,"merged":[[1,0,1,8],[2,0,2,8],[4,0,7,0],[8,0,9,0],[11,0,11,8],[15,0,15,7]]}
["附件1："]
["重庆农投集团信息系统整体云托管服务报价明细表"]
["一、基础产品服务"]
["类型","产品名称","规格","操作系统","云配置具体配置要求","数量","单价（元/年）","总价（元/年）","备注"]
["云主机","财务系统应用服务器","4核 8GB","windows server\n2012 R2以上","系统盘60G，数据盘100G。\nCPU频率：供应商填写",1]
[null,"财务系统数据库服务器","16核32GB","windows server\n2012 R2以上","系统盘60G，数据盘500G\nCPU频率：供应商填写",1]
[null,"官网和OA系统应用服务器","32核32G","windows server\n2012 R2以上","系统盘200G，数据盘1848G\nCPU频率：供应商填写",1]
[null,"OA数据库服务器","16核32G","windows server\n2012 R2以上","系统盘200G，数据盘824G\nCPU频率：供应商填写",1]
["云网络","弹性公网IP","EIP（多线BGP 50M共享公网带宽）    ",null,null,1]
[null,"VPN专用通道","VPN网关（Ipsec-VPN 带宽：10M   ）",null,null,1]
["小计"]
["二、安全及备份"]
["云安全","主机安全",{"$nulls":6},"根据主机实际情况配置安全产品，由服务商自行填写。"]
["备份","云服务器备份",{"$nulls":6},"根据主机实际情况配置备份产品，由服务商自行填写。"]
["小计"]
["          三、三级等保测评安全产品"]
["安全",{"$nulls":7},"根据三级等级保护测评要求配置安全产品，由服务商填写。"]
["小计"]
["总计"]